/* These are the newlib functions present in ESP32 ROM.
   They should not be used when you need to solve the Y2K38 problem.
   Because these functions were compiled with 32-bit width for the time_t structure.
 */

asctime = 0x40059588;
asctime_r = 0x40000ec8;
ctime = 0x400595b0;
ctime_r = 0x400595c4;
__gettzinfo = 0x40001fcc;
__get_current_time_locale = 0x40001834;
gmtime = 0x40059848;
gmtime_r = 0x40059868;
localtime = 0x400595dc;
localtime_r = 0x400595fc;
mktime = 0x4005a5e8;
strftime = 0x40059ab4;
time = 0x40001844;
__time_load_locale = 0x4000183c;
tzset = 0x40001a1c;
_tzset_r = 0x40001a28;
