# Override some defaults so BT stack is enabled
# in this example

#
# BT config
#
CONFIG_BT_ENABLED=y
CONFIG_BTDM_CTRL_MODE_BLE_ONLY=y
CONFIG_BTDM_CTRL_MODE_BR_EDR_ONLY=n
CONFIG_BTDM_CTRL_MODE_BTDM=n
CONFIG_BT_BLUEDROID_ENABLED=n
CONFIG_BT_NIMBLE_ENABLED=y

# Enable support for power management
CONFIG_PM_ENABLE=y
# Enable tickless idle mode
CONFIG_FREERTOS_USE_TICKLESS_IDLE=y
# Set the tick rate at which FreeRTOS does pre-emptive context switching.
CONFIG_FREERTOS_HZ=1000
# Minimum number of ticks to enter sleep mode for
CONFIG_FREERTOS_IDLE_TIME_BEFORE_SLEEP=3
CONFIG_FREERTOS_TIMER_TASK_STACK_DEPTH=4000
