# Place FreeRTOS functions into flash to save some IRAM on the ESP32
CONFIG_FREERTOS_PLACE_FUNCTIONS_INTO_FLASH=y
# Use the SINGLE_APP_LARGE partition to ensure the partition has enough space for the ESP32 build
CONFIG_PARTITION_TABLE_SINGLE_APP_LARGE=y
