# Override some defaults so BT stack is enabled
# by default in this example
CONFIG_IDF_TARGET="esp32s3"
CONFIG_BT_CTRL_SCAN_DUPL_TYPE_DATA_DEVICE=y
CONFIG_BT_CTRL_BLE_MESH_SCAN_DUPL_EN=y
CONFIG_BT_BLE_42_FEATURES_SUPPORTED=y
CONFIG_BT_BLE_50_FEATURES_SUPPORTED=n

#
# light driver config
#
CONFIG_LIGHT_GPIO_RED=14
CONFIG_LIGHT_GPIO_GREEN=13
CONFIG_LIGHT_GPIO_BLUE=12
CONFIG_LIGHT_GPIO_COLD=11
CONFIG_LIGHT_GPIO_WARM=10
# end of light driver config
