# Override some defaults so BT stack is enabled
# by default in this example
CONFIG_IDF_TARGET="esp32s3"
CONFIG_BT_CTRL_SCAN_DUPL_TYPE_DATA_DEVICE=y
CONFIG_BT_CTRL_BLE_MESH_SCAN_DUPL_EN=y
CONFIG_BT_BLE_42_FEATURES_SUPPORTED=y
CONFIG_BT_BLE_50_FEATURES_SUPPORTED=n

CONFIG_ESP_DEFAULT_CPU_FREQ_MHZ_240=y
CONFIG_ESP_DEFAULT_CPU_FREQ_MHZ=240
