/*  Default entry point:  */
ENTRY(call_start_cpu0);

SECTIONS
{
  /* RTC fast memory holds RTC wake stub code,
     including from any source file named rtc_wake_stub*.c
  */
  .rtc.text :
  {
    . = ALIGN(4);
    *(.rtc.literal .rtc.text)
    *rtc_wake_stub*.*(.literal .text .literal.* .text.*)
  } > rtc_iram_seg

  /* RTC slow memory holds RTC wake stub
     data/rodata, including from any source file
     named rtc_wake_stub*.c
  */
  .rtc.data :
  {
    _rtc_data_start = ABSOLUTE(.);
    *(.rtc.data)
    *(.rtc.rodata)
    *rtc_wake_stub*.*(.data .rodata .data.* .rodata.* .bss .bss.*)
    _rtc_data_end = ABSOLUTE(.);
  } > rtc_slow_seg

  /* RTC bss, from any source file named rtc_wake_stub*.c */
  .rtc.bss (NOLOAD) :
  {
    _rtc_bss_start = ABSOLUTE(.);
    *rtc_wake_stub*.*(.bss .bss.*)
    *rtc_wake_stub*.*(COMMON)
    _rtc_bss_end = ABSOLUTE(.);
  } > rtc_slow_seg

  /* This section holds data that should not be initialized at power up 
     and will be retained during deep sleep. The section located in 
     RTC SLOW Memory area. User data marked with RTC_NOINIT_ATTR will be placed
     into this section. See the file "esp_attr.h" for more information.
  */
  .rtc_noinit (NOLOAD):
  {
    . = ALIGN(4);
    _rtc_noinit_start = ABSOLUTE(.);
    *(.rtc_noinit .rtc_noinit.*)
    . = ALIGN(4) ;
    _rtc_noinit_end = ABSOLUTE(.);
  } > rtc_slow_seg

  /* Send .iram0 code to iram */
  .iram0.vectors :
  {
    /* Vectors go to IRAM */
    _init_start = ABSOLUTE(.);
    /* Vectors according to builds/RF-2015.2-win32/esp108_v1_2_s5_512int_2/config.html */
    . = 0x0;
    KEEP(*(.WindowVectors.text));
    . = 0x180;
    KEEP(*(.Level2InterruptVector.text));
    . = 0x1c0;
    KEEP(*(.Level3InterruptVector.text));
    . = 0x200;
    KEEP(*(.Level4InterruptVector.text));
    . = 0x240;
    KEEP(*(.Level5InterruptVector.text));
    . = 0x280;
    KEEP(*(.DebugExceptionVector.text));
    . = 0x2c0;
    KEEP(*(.NMIExceptionVector.text));
    . = 0x300;
    KEEP(*(.KernelExceptionVector.text));
    . = 0x340;
    KEEP(*(.UserExceptionVector.text));
    . = 0x3C0;
    KEEP(*(.DoubleExceptionVector.text));
    . = 0x400;
    *(.*Vector.literal)

    *(.UserEnter.literal);
    *(.UserEnter.text);
    . = ALIGN (16);
    *(.entry.text)
    *(.init.literal)
    *(.init)
    _init_end = ABSOLUTE(.);

    /* This goes here, not at top of linker script, so addr2line finds it last,
       and uses it in preference to the first symbol in IRAM */
    _iram_start = ABSOLUTE(0);
  } > iram0_0_seg

  .iram0.text :
  {
    /* Code marked as runnning out of IRAM */
    _iram_text_start = ABSOLUTE(.);
    *(.iram1 .iram1.*)
    *libfreertos.a:(.literal .text .literal.* .text.*)
    *libheap.a:multi_heap.*(.literal .text .literal.* .text.*)
    *libheap.a:multi_heap_poisoning.*(.literal .text .literal.* .text.*)
    *libesp32.a:panic.*(.literal .text .literal.* .text.*)
    *libesp32.a:core_dump.*(.literal .text .literal.* .text.*)
    *libapp_trace.a:(.literal .text .literal.* .text.*)
    *libxtensa-debug-module.a:eri.*(.literal .text .literal.* .text.*)
    *librtc.a:(.literal .text .literal.* .text.*)
    *libsoc.a:(.literal .text .literal.* .text.*)
    *libhal.a:(.literal .text .literal.* .text.*)
    *libgcc.a:lib2funcs.*(.literal .text .literal.* .text.*)
    *libspi_flash.a:spi_flash_rom_patch.*(.literal .text .literal.* .text.*)
    *libgcov.a:(.literal .text .literal.* .text.*)
    INCLUDE esp32.spiram.rom-functions-iram.ld
    _iram_text_end = ABSOLUTE(.);
  } > iram0_0_seg
  
  .dram0.data :
  {
    _data_start = ABSOLUTE(.);
    *(.data)
    *(.data.*)
    *(.gnu.linkonce.d.*)
    *(.data1)
    *(.sdata)
    *(.sdata.*)
    *(.gnu.linkonce.s.*)
    *(.sdata2)
    *(.sdata2.*)
    *(.gnu.linkonce.s2.*)
    *(.jcr)
    *(.dram1 .dram1.*)
    *libesp32.a:panic.*(.rodata .rodata.*)
    *libphy.a:(.rodata .rodata.*)
    *libsoc.a:rtc_clk.*(.rodata .rodata.*)
    *libapp_trace.a:(.rodata .rodata.*)
    *libgcov.a:(.rodata .rodata.*)
    *libheap.a:multi_heap.*(.rodata .rodata.*)
    *libheap.a:multi_heap_poisoning.*(.rodata .rodata.*)
    INCLUDE esp32.spiram.rom-functions-dram.ld
    _data_end = ABSOLUTE(.);
    . = ALIGN(4);
  } > dram0_0_seg

  /*This section holds data that should not be initialized at power up.
    The section located in Internal SRAM memory region. The macro _NOINIT
    can be used as attribute to place data into this section.
    See the esp_attr.h file for more information.
  */
  .noinit (NOLOAD):
  {
    . = ALIGN(4);
    _noinit_start = ABSOLUTE(.);
    *(.noinit .noinit.*) 
    . = ALIGN(4) ;
    _noinit_end = ABSOLUTE(.);
  } > dram0_0_seg

  /* Shared RAM */
  .dram0.bss (NOLOAD) :
  {
    . = ALIGN (8);
    _bss_start = ABSOLUTE(.);
    *(.dynsbss)
    *(.sbss)
    *(.sbss.*)
    *(.gnu.linkonce.sb.*)
    *(.scommon)
    *(.sbss2)
    *(.sbss2.*)
    *(.gnu.linkonce.sb2.*)
    *(.dynbss)
    *(.bss)
    *(.bss.*)
    *(.share.mem)
    *(.gnu.linkonce.b.*)
    *(COMMON)
    . = ALIGN (8);
    _bss_end = ABSOLUTE(.);
    /* The heap starts right after end of this section */
    _heap_start = ABSOLUTE(.);
  } > dram0_0_seg

  .flash.rodata :
  {
    _rodata_start = ABSOLUTE(.);
    *(.rodata)
    *(.rodata.*)
    *(.irom1.text) /* catch stray ICACHE_RODATA_ATTR */
    *(.gnu.linkonce.r.*)
    *(.rodata1)
    __XT_EXCEPTION_TABLE_ = ABSOLUTE(.);
    *(.xt_except_table)
    *(.gcc_except_table .gcc_except_table.*)
    *(.gnu.linkonce.e.*)
    *(.gnu.version_r)
    . = (. + 3) & ~ 3;
    __eh_frame = ABSOLUTE(.);
    KEEP(*(.eh_frame))
    . = (. + 7) & ~ 3;
    /*  C++ constructor and destructor tables, properly ordered:  */
    __init_array_start = ABSOLUTE(.);
    KEEP (*crtbegin.*(.ctors))
    KEEP (*(EXCLUDE_FILE (*crtend.*) .ctors))
    KEEP (*(SORT(.ctors.*)))
    KEEP (*(.ctors))
    __init_array_end = ABSOLUTE(.);
    KEEP (*crtbegin.*(.dtors))
    KEEP (*(EXCLUDE_FILE (*crtend.*) .dtors))
    KEEP (*(SORT(.dtors.*)))
    KEEP (*(.dtors))
    /*  C++ exception handlers table:  */
    __XT_EXCEPTION_DESCS_ = ABSOLUTE(.);
    *(.xt_except_desc)
    *(.gnu.linkonce.h.*)
    __XT_EXCEPTION_DESCS_END__ = ABSOLUTE(.);
    *(.xt_except_desc_end)
    *(.dynamic)
    *(.gnu.version_d)
    _rodata_end = ABSOLUTE(.);
    /* Literals are also RO data. */
    _lit4_start = ABSOLUTE(.);
    *(*.lit4)
    *(.lit4.*)
    *(.gnu.linkonce.lit4.*)
    _lit4_end = ABSOLUTE(.);
    . = ALIGN(4);
    _thread_local_start = ABSOLUTE(.);
    *(.tdata)
    *(.tdata.*)
    *(.tbss)
    *(.tbss.*)
    _thread_local_end = ABSOLUTE(.);
    . = ALIGN(4);
  } >drom0_0_seg

  .flash.text :
  {
    _stext = .;
    _text_start = ABSOLUTE(.);
    *(.literal .text .literal.* .text.* .stub .gnu.warning .gnu.linkonce.literal.* .gnu.linkonce.t.*.literal .gnu.linkonce.t.*)
    *(.irom0.text) /* catch stray ICACHE_RODATA_ATTR */
    *(.fini.literal)
    *(.fini)
    *(.gnu.version)
    _text_end = ABSOLUTE(.);
    _etext = .;

    /* Similar to _iram_start, this symbol goes here so it is
       resolved by addr2line in preference to the first symbol in
       the flash.text segment.
    */
    _flash_cache_start = ABSOLUTE(0);
  } >iram0_2_seg
}
