if ESP_EVENT_POST_FROM_IRAM_ISR = y:
    [mapping:esp_event]
    archive: libesp_event.a
    entries:
        esp_event:esp_event_isr_post_to (noflash)
        default_event_loop:esp_event_isr_post (noflash)
