# This file was generated using idf.py save-defconfig. It can be edited manually.
# Espressif IoT Development Framework (ESP-IDF) 5.4.1 Project Minimal Configuration
#
CONFIG_BOOTLOADER_APP_ROLLBACK_ENABLE=y
CONFIG_APP_PROJECT_VER_FROM_CONFIG=y
CONFIG_APP_PROJECT_VER="v4.1.0.0-dev"
CONFIG_ESPTOOLPY_FLASHSIZE_4MB=y
CONFIG_PARTITION_TABLE_CUSTOM=y
CONFIG_PARTITION_TABLE_CUSTOM_FILENAME="module_config/module_esp32_default/partitions_at.csv"
CONFIG_PARTITION_TABLE_MD5=n
CONFIG_AT_CUSTOMIZED_PARTITION_TABLE_FILE="module_config/module_esp32_default/at_customize.csv"
CONFIG_BT_ENABLED=y
CONFIG_BT_BTU_TASK_STACK_SIZE=5120
CONFIG_BT_BLE_BLUFI_ENABLE=y
CONFIG_BT_STACK_NO_LOG=y
CONFIG_BT_BLE_DYNAMIC_ENV_MEMORY=y
CONFIG_BTDM_CTRL_MODE_BTDM=y
CONFIG_BTDM_CTRL_LPCLK_SEL_EXT_32K_XTAL=y
CONFIG_BTDM_SCAN_DUPL_CACHE_SIZE=200
CONFIG_ESP_TLS_PSK_VERIFICATION=y
CONFIG_ESP_TLS_INSECURE=y
CONFIG_ESP_TLS_SKIP_SERVER_CERT_VERIFY=y
CONFIG_ESP_ERR_TO_NAME_LOOKUP=n
CONFIG_GPIO_ESP32_SUPPORT_SWITCH_SLP_PULL=y
CONFIG_ETH_DMA_RX_BUFFER_NUM=3
CONFIG_ETH_DMA_TX_BUFFER_NUM=3
CONFIG_HTTPD_MAX_REQ_HDR_LEN=1024
CONFIG_HTTPD_MAX_URI_LEN=1024
CONFIG_ESP_HTTPS_OTA_ALLOW_HTTP=y
CONFIG_RTC_CLK_SRC_EXT_CRYS=y
CONFIG_RTC_EXT_CRYST_ADDIT_CURRENT=y
CONFIG_RTC_CLK_CAL_CYCLES=1024
CONFIG_PM_ENABLE=y
CONFIG_PM_SLP_DISABLE_GPIO=y
CONFIG_ESP_DEFAULT_CPU_FREQ_MHZ_80=y
CONFIG_ESP_TASK_WDT_PANIC=y
CONFIG_ESP_TASK_WDT_TIMEOUT_S=60
CONFIG_ESP_DEBUG_OCDAWARE=n
CONFIG_ESP_WIFI_IRAM_OPT=n
CONFIG_ESP_WIFI_RX_IRAM_OPT=n
CONFIG_ESP_WIFI_SLP_IRAM_OPT=y
CONFIG_ESP_WIFI_SLP_BEACON_LOST_OPT=y
CONFIG_ESP_WIFI_ESPNOW_MAX_ENCRYPT_NUM=0
CONFIG_FATFS_LFN_HEAP=y
CONFIG_FREERTOS_UNICORE=y
CONFIG_FREERTOS_HZ=1000
CONFIG_FREERTOS_USE_TICKLESS_IDLE=y
CONFIG_FREERTOS_CHECK_MUTEX_GIVEN_BY_OWNER=n
CONFIG_FREERTOS_PLACE_FUNCTIONS_INTO_FLASH=y
CONFIG_HEAP_PLACE_FUNCTION_INTO_FLASH=y
CONFIG_LOG_DEFAULT_LEVEL_ERROR=y
CONFIG_LWIP_MAX_SOCKETS=16
CONFIG_LWIP_SO_LINGER=y
CONFIG_LWIP_SO_RCVBUF=y
CONFIG_LWIP_IP4_REASSEMBLY=y
CONFIG_LWIP_IP6_REASSEMBLY=y
CONFIG_LWIP_IPV6_AUTOCONFIG=y
CONFIG_LWIP_TCP_MAXRTX=6
CONFIG_LWIP_TCP_SYNMAXRTX=3
CONFIG_LWIP_PPP_SUPPORT=y
CONFIG_LWIP_PPP_SERVER_SUPPORT=y
CONFIG_LWIP_SNTP_MAX_SERVERS=3
CONFIG_LWIP_SNTP_STARTUP_DELAY=n
CONFIG_MBEDTLS_DYNAMIC_BUFFER=y
CONFIG_MBEDTLS_DYNAMIC_FREE_CONFIG_DATA=y
CONFIG_MBEDTLS_SSL_KEEP_PEER_CERTIFICATE=n
CONFIG_MBEDTLS_HAVE_TIME_DATE=y
CONFIG_MBEDTLS_DHM_C=y
CONFIG_NEWLIB_NANO_FORMAT=y
CONFIG_VFS_SUPPORT_TERMIOS=n
CONFIG_WL_SECTOR_SIZE_512=y
CONFIG_AT_PROCESS_TASK_STACK_SIZE=6144
CONFIG_AT_MQTT_COMMAND_SUPPORT=y
CONFIG_AT_HTTP_COMMAND_SUPPORT=y
CONFIG_AT_BLE_COMMAND_SUPPORT=n
CONFIG_AT_BLE_HID_COMMAND_SUPPORT=n
CONFIG_AT_BLUFI_COMMAND_SUPPORT=n
