# Copyright (C) Ivan Kravets <me@ikravets.com>
# See LICENSE for details.

# UDEV Rules for PlatformIO supproted boards, http://platformio.org/#!/boards
#
# The latest version of this file may be found at:
# 	https://github.com/platformio/platformio/blob/develop/scripts/99-platformio-udev.rules
#
# This file must be placed at:
# 	/etc/udev/rules.d/99-platformio-udev.rules    (preferred location)
#   	or
# 	/lib/udev/rules.d/99-platformio-udev.rules    (req'd on some broken systems)
#
# To install, type this command in a terminal:
# 	sudo cp 99-platformio-udev.rules /etc/udev/rules.d/99-platformio-udev.rules
#
# Restart "udev" management tool:
#	sudo service udev restart
#		or
# 	sudo udevadm control --reload-rules
#	sudo udevadm trigger
#
# After this file is installed, physically unplug and reconnect your board.

# CP210X USB UART
SUBSYSTEMS=="usb", ATTRS{idVendor}=="10c4", ATTRS{idProduct}=="ea60", MODE:="0666"

# FT232R USB UART
SUBSYSTEMS=="usb", ATTRS{idVendor}=="0403", ATTRS{idProduct}=="6001", MODE:="0666"

# Prolific Technology, Inc. PL2303 Serial Port
SUBSYSTEMS=="usb", ATTRS{idVendor}=="067b", ATTRS{idProduct}=="2303", MODE:="0666"

# QinHeng Electronics HL-340 USB-Serial adapter
SUBSYSTEMS=="usb", ATTRS{idVendor}=="1a86", ATTRS{idProduct}=="7523", MODE:="0666"

# ARDUINO UNO
SUBSYSTEMS=="usb", ATTRS{idVendor}=="2341", ATTRS{idProduct}=="0043", MODE:="0666"

# Digistump boards
SUBSYSTEMS=="usb", ATTRS{idVendor}=="16d0", ATTRS{idProduct}=="0753", MODE:="0666"
KERNEL=="ttyACM*", ATTRS{idVendor}=="16d0", ATTRS{idProduct}=="0753", MODE:="0666", ENV{ID_MM_DEVICE_IGNORE}="1"

# STM32 discovery boards, with onboard st/linkv2
SUBSYSTEMS=="usb", ATTRS{idVendor}=="0483", ATTRS{idProduct}=="3748", MODE:="0666"

# USBtiny
SUBSYSTEMS=="usb", ATTRS{idProduct}=="0c9f", ATTRS{idVendor}=="1781", MODE="0666"

# Teensy boards
ATTRS{idVendor}=="16c0", ATTRS{idProduct}=="04[789]?", ENV{ID_MM_DEVICE_IGNORE}="1"
ATTRS{idVendor}=="16c0", ATTRS{idProduct}=="04[789]?", ENV{MTP_NO_PROBE}="1"
SUBSYSTEMS=="usb", ATTRS{idVendor}=="16c0", ATTRS{idProduct}=="04[789]?", MODE:="0666"
KERNEL=="ttyACM*", ATTRS{idVendor}=="16c0", ATTRS{idProduct}=="04[789]?", MODE:="0666"

#TI Stellaris Launchpad
SUBSYSTEMS=="usb", ATTRS{idVendor}=="1cbe", ATTRS{idProduct}=="00fd", MODE="0666"

#TI MSP430 Launchpad
SUBSYSTEMS=="usb", ATTRS{idVendor}=="0451", ATTRS{idProduct}=="f432", MODE="0666"
